** Emergency Shower Station
 Weekly Inspection Checklist**

**How to obtain assistance:**

**Questions, maintenance requests, training information**

Environmental Health and Safety: 5-5448

**Maintenance requests may also be called in directly**

Service Desk: 5-5050

Facilities Services (Zone Maintenance): Zone A: 5-3730

Zone B: 5-6173 Zone D: 5-3414 Zone E: 5-2968

Zone F: 5-7354

**Emergencies:**

Immediately stand in the water stream and flush the affected area for 15 minutes. Remove contaminated clothing while showering and not before. CALL 911 and seek medical assistance.

**How to Test:**

* Is access to the shower free of obstructions from all areas of the laboratory or hallway?
* Place a 5-gallon bucket underneath the safety shower and a shower curtain around the shower head and inside the bucket to catch all the water (Note: the shower will produce 20 gallons/minute)
* Evaluate for adequate flow
* Does the water continue to flow until the pull handle is turned off?
* Is the plumbing free from leakage?

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Date** | **Initials** | **Comment** |  | **Date** | **Initials** | **Comment** |  | **Date** | **Initials** | **Comment** |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |